{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["Calculations","Documentation"],"not_rendered":{"charts":0,"images":2,"macros":1,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Calculations","index":0,"n_rows":9,"n_cols":2,"rows_kept":9,"cut":false,"hidden":false,"merged":[]}
["Measurements in Inches"]
["Catch Basin Inside Width",48]
["Cath Basin Wall Thickness",8]
[]
["Inside Diameter of Pipe",18]
["Minimum Depth of Cover",23]
["Slope (X:1)",24]
[]
["Minumim Design Depth",3.9034285371192978]

{"sheet":"Documentation","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}